040-64557365
Fire Detection & Alarm System
Fire Detection and Alarm system consist of smoke detectors and manual call point placed at strategic location and connected by cabling through a control panel. The purpose of Fire Alarm System is to detect fire as earliest practicable moment and give an alarm so that appropriate action can be taken to prevent outbreak of Fire. The Alarm systems can also be used for Alarming and evacuation of people, remote alarm generation at fire stations. Fire detector detects the presence of heat or smoke generated during the early stages of fire and gives an alarm signal to the control panel. Intelligent Addressable: Intelligent Addressable Systems offer benefits in terms of speed of detection, identification of the pin point location of Fire and easier maintenance. Intelligent systems also offer tolerance to faults in the system wiring, which allows a single pair of wires to be used to connect up to 250 devices to the system, cost savings in the wiring of large systems. Conventional: Conventional Fire Alarm System provides the earliest practicable fire detection and warning. This system consists of smoke or heat detectors at designated locations, to detect smoke or heat at the earliest during any outbreak of fire. Conventional Fire Alarm System Intelligent addressable Fire alarm system Wireless/ Standalone Fire Alarm System Aspiration System Water Leak Detection System Temperature Monitoring System
Top
Fire Hydrant & Sprinkler system
Water Based Systems
SBE Fire Solution offers a range of Water Based Fire Protection Systems like Sprinkler, Hydrant, Pre-action Systems, High and Medium Velocity Systems and Tank Foam System to suit individual Fire protection needs. Stopping a fire early can save lives and assets. In fire protection, you would want all the effectiveness you can get, as fast as you can get it. At SBE Fire Solutions, our complete range of products and services are designed to ensure fire detection and protection for all types of fire risks. We are committed to delivering solutions that meet your business and protection needs. We are ready to work with you to protect your people, property and assets, 24 hours a day, 7 days a week, and 365 days a year. Sprinklers are the most widely used fire protection system in the world today. They provide effective control over fire when installed according to the requirements of local fire codes. There are many different types of sprinklers, each built for use against different types of fire risks. Ongoing research and development ensures that newer and more reliable sprinklers are constantly being developed. Together with active alarms and simultaneous alerts to fire brigades, sprinklers provide fast and effective fire suppression in the entire integrated fire response system.
Fire Hydrant
Sprinkler System
Gas/Foam Based Systems
In addition to Fire detection and alarm systems, organizations that have a dedicated server / rack rooms MSC, Data Centre should have minimum gas suppression systems. The different types of gas suppression systems available are FM-200 and Inergen.
Top
Surveillance System: CCTV
Closed Circuit Television is now widely accepted as the 'first line' of defense for personnel and premise security. When cameras are properly targeted, they can deter offenders, reduce the level of crime and increase the feeling of safety in the controlled area. CCTV solutions, or video surveillance solutions, are now considered to be an integral part of most security systems. Fire Solution provides design, installation, support, monitoring services - and integration - of CCTV solutions, including all key video systems components and concepts: CCTV cameras (including IP, infrared, low-light, pinhole, waterproof, mini, dome) DVR (digital video recorder) NVSR (Network video Server recorder) Fiber optic / Networked / IP transmission Networked CCTV transmission (IP CCTV transmission) Software systems for CCTV control, CCTV Management and CCTV diagnostics
Access Control System
The Access Control forms a security barrier and hence protects the facilities from unauthorized entries. Every individual working in the facility has unique cards hence trespassing is avoided. The Access can be controlled through various mechanisms such as door locks, turnstiles, sliding doors, retractable barriers and swing gates among others, based on the level of security desired. The basic system will have a reader request to exit switch, lock or turnstile or any other barrier, controller to control all these devices and software for generation of various reports. Today's multi-site, access/ID solutions have changed the way security, property and even HR managers look at access control systems. By providing a fully-integrated, centralized, networked access control solution organization accountability is now achievable. Access control means different things to different customers. It can cover a spectrum of capabilities including concepts and elements such as: ID cards Proximity cards, Mag-stripe swipe cards Smart cards, Keypads Biometrics Centralized management, control and reporting Remote access Time and attendance system Types of Access Control System: Standalone Access Control system Intelligent Access Control system Boom Barrier, Turnstile, Tripod and Flap Barrier Global Proprietary Access Control system
Public Address System
A multi application PA Amplifier capable of delivering 200+200 Watts output. Ideal for PA Installations in mosque, temples and other religious places, as well as for other indoor and outdoor sound reinforcement applications. This amplifier has a built-in MP3 player with USB, SD and MMC card reader, which is ideal for DJ's and stereo music applications for various gatherings. This amplifier is designed to give clean sound and reliable, trouble free operation under severe climatic conditions. Features includes 6 Mics, 2 Aux. Inputs and RCA jacks at rear for CD/DVD players. In addition, resettable circuit protector, ±10dB Cut/Boost Bass and Treble Controls and AC/24 Volts Battery operation are provided.
Process Control Instrumentation products
1. Temperature Indicators & Controllers (Flame Proof & Non Flame Proof) 2. PID Controllers & Programmers. 3. Scanners &Data loggers, Humidity Transmitters 4. Thermocouples & RTD’s (Flame Proof & Non Flame Proof) 5. Temperature Recorders 6. Pressure Transmitters & DP Transmitters 7. Temperature Transmitters 8. Pressure Gauges, Counters 9. Dead Weight Pressure Gauge Tester 10. Flow meters 11. I/P Converters 12. SCADA Software 13. AC Drives 15. Universal Calibrators 16. Strip Chart Recorder Consumables 17. Control valves 18. Pressure Calibrators 19. Temperature dry block Calibrators 20. Portable Flue gas Analyzers, Dew point transmitters, Infrared thermometers, Thermal Imagers, Air velocity measuring instruments, Sound Level meters, RH & Temp Measuring Instruments, wireless Data loggers, Manometers etc 21. Level-Guided & Non –guided Radar type Level transmitters, Ultrasonic Level Transmitter, Capacitance type Level transmitter Magnostric Level transmitter, Conductivity type level switches, magnetic type float level switches, vibrating type level switches etc 22. Temperature Switches 23. Thermal Image 875-2,875-1,880-3 24. Flue Gas Analyzer
GIS-Photo-geometry
Top
Gis Earth Solution: GIS Application Development, GeoSpatial Data Modeling & Geodatabase Design, GIS Software Implementation | Photogrammetry is the first remote sensing technology ever developed, in which geometric properties about objects are determined from photographic images.